**Trailer Setup Steps**

1. **Chock Wheels** and disconnect trailer from Truck.
2. Level trailer with Jacks.
3. Hook up LP and Battery
4. Unhook four roof release locks. Crank up until Green Cable is JUST taunt.
5. Slide each end out, put 2 braces under slide outs on each end.
6. Attach all bungee cords underneath end bunks (12 total)
7. Put 2 safety braces in opposite corners on lifting tubes. Pull canvas over Tubes.
8. Setup Trailer Step by pulling out.
9. Push End Rafters over bunks up from the inside; add top braces on each end.
10. Move Stove outside Put Cushions in Place, put tables in Place.
11. Unhook the door from the ceiling, lock bottom of door, Velcro around frame.
12. Connect Water, Electric, check for leaks.
13. Start Fridge on 110v, 12v, or Propane as needed

**Trailer Take down Steps**

1. Disconnect Water and 110v power, turn off refrigerator.
2. Stow electric cord, water hose and fittings.
3. Switch lighting inside to 12v with switch under front dinette.
4. Unlatch Door, release Velcro and swing up lock to roof.
5. Zip all windows shut to protect screens.
6. Remove End Rafter Braces, drop end rafters down.
7. Put stove on floor between dinette on back end on top of rug.
8. Fold down table tops and stow cushions
9. Shut off all inside lighting (can’t reach it soon)
10. Tip sink over to transit position, put leg on front of sink down.
11. Remove four outside underside Bunk Braces and stow.
12. Remove Raise tube braces (2 of these) and stow.
13. Push Step in.
14. Unhook Bungee cords underneath bunks (12 of them)
15. Slide Bunk ends in.
16. Lower roof tucking canvas as it goes, finally locking in place with 4 corner locks.
17. Pull Crank and stow inside.
18. Lift the jacks on rear of trailer, connect to truck, check lights.
19. Shut off LP, remove wheel chocks and stow.
20. Perform walk around prior to departure.